**CC 380SH Feature List (2 axle)**

* Tandem Demolition Trailer
* 1/4: Hardox 450 Tub
* 84 cubic yard capacity
* 101" sidewall height
* 2 speed landing gear
* Hutch H900-OS single point suspension
* 50" axle spacing
* Unimont w/ Long studs
* 24.5 " cooper road master tires
* Mud flaps on tail gate
* Side swing tailgate
* Standard LED lighting
* White steel inner and outer wheels
* Four on the floor